SECTION 1:     CHEMICAL AND MANUFACTURER IDENTIFICATION
Product Name: BrilloDuro Triple-9 Tan Base Coat A    Product Code: 0365F210

Manufactured For:
Action Industrial Coatings, LLC
3463 N. Gillett St
Appleton, WI 54914
(920) 470-0838

24 Hour Emergency:  INFOTRAC: 1-800-535-5053

Outside U.S. and Canada:  Infotrac: 352-323-3500

INFOTRAC Customer ID: 72826

NOTE: INFOTRAC and National Response Center 
emergency numbers to be used only in the event 
of chemical emergencies involving a spill, leak, fire, 
exposure or accident involving chemicals
Not recommended for: 
Because many of the conditions are within the user's knowledge and control, it is essential that the user evaluate and determine whether the product is suitable and appropriate for a particular use and intended application, and complies with all local applicable laws, regulations, standards, and guidance.
SECTION 2:     HAZARD(S) IDENTIFICATION

Prepared according to Global Harmonized System (GHS) Standards

GHS Classification Scale                 1=Severe Hazard; 4=Slight Hazard

GHS Ratings:
There are no GHS ratings that apply to this product at this time
GHS Hazards
There are no GHS hazards that apply to this product at this time
GHS Precautions
There are no GHS precautions that apply to this product at this time
SECTION 3:     COMPOSITION / INFORMATION ON INGREDIENTS
Chemical Name 
CAS number
Weight Concentration %
Titanium dioxide
13463-67-7
10.00% - 20.00%
Solvent naphtha, petroleum, light aromatic
64742-95-6
0.10% - 1.00%
SECTION 4:     FIRST AID MEASURES
SDS for:  0365F210
Page 1 of 6
Printed:  6/21/2023 at  4:20:45PM

Inhalation:  Move affected person to fresh air. If breathing has stopped, administer CPR. If the person vomits, clean the airway and turn their head to the side to prevent choking. If the person is unconscious but breathing, place them stably on their left side in the recovery position. Never give anything by mouth to an unconscious person. Seek immediate medical attention.

Eyes:  Flush eyes gently with clean water for at least 15 minutes. If irritation persists, seek immediate medical attention.

Skin:  Remove any contaminated clothing using appropriate gloves. Rinse skin thoroughly for 15 minutes in a shower or with a hose. Seek immediate medical attention.

Ingestion:  Rinse mouth with water to remove any residual chemical. If the person vomits, clean their airway and turn their head to the side to prevent choking. DO NOT induce vomiting and DO NOT give them anything to drink unless directed to do so by a physician. If the person is unconscious but breathing, place them stably on their left side in recovery position. Never give anything by mouth to an unconscious person. Seek immediate medical attention.

Additional Notes to Physician - Treat symptomatically. No specific antidote available
SECTION 5:     FIREFIGHTING MEASURES
Flash Point: N/A
LEL: N/A
UEL: N/A

Suitable Extinguishing Media:  
Foam
Carbon Dioxide (CO2)
Dry Chemical
Specific Hazards During Firefighting:  Prevent firefighting run-off from entering drains or sewers.

Byproducts of Combustion:  Fires involving this product may release oxides of carbon and nitrogen, reactive hydrocarbons, and irritating vapors.

Unusual Fire and Explosion Hazards:  Any closed container may rupture when exposed to extreme heat. Use a water spray to cool sealed containers. Solvent vapors are heavier than air and can travel along the ground. 

SECTION 6:     ACCIDENTAL RELEASE MEASURES

Spill / Leak Clean-Up Procedures:
 
Immediately turn off or isolate any source of ignition (pilot lights, electrical equipment, flames, heaters, etc.). Evacuate area and ventilate. Personnel wearing proper protective equipment should contain spill immediately with inert materials (sand, earth, chemical spill pads of cotton) by forming dikes. Dikes should be placed to contain spill in a manner that will prevent material from entering sewers and waterways. Large spills, once contained, may be picked up using explosion proof, non-sparking vacuum pumps, shovels, or buckets, and disposed of in suitable containers. If a large spill occurs notify the appropriate authorities. 

In case of road spill or accident contact INFOTRAC (1-800-535-5053).

CAUTION:  If spilled material is cleaned up using a regulated solvent, the resulting waste mixture will also be regulated.

Do not empty into drains. All disposal must comply with federal, state, and local regulations. The material, if spilled or discarded, may be a regulated waste. Refer to state and local regulations. Department of Transportation (DOT) regulations may apply for transporting this material when spilled. See Section 14.

SDS for:  0365F210
Page 2 of 6
Printed:  6/21/2023 at  4:20:45PM

SECTION 7:     HANDLING AND STORAGE

Handling Precautions:  

Open containers carefully and in a well ventilated area, and use appropriate respiratory protection. Wash hands thoroughly after handling. Keep containers closed when not in use. Do not transfer to unmarked containers. Empty containers contain product residue which may exhibit hazardous properties therefore, do not pressurize, cut, glaze, weld or use for any other purpose. Return drums to reclamation center for proper cleaning and reuse.

Storage Requirements:
  
Store in a cool, dry, well ventilated area. Keep containers tightly closed and store away from heat, sparks, open flame or oxidizing materials. Extended storage at excessive temperatures may produce odorous and toxic fumes from product decomposition.

SECTION 8:     EXPOSURE CONTROLS / PERSONAL PROTECTION
Other Exposure Limits
ACGIH Exposure Limits
OSHA Exposure Limits
Chemical Name / CAS No.
Titanium dioxide
13463-67-7
10 mg/m3 TWA
15 mg/m3 TWA (total dust)
Not Established
Solvent naphtha, petroleum, light aromatic
64742-95-6
Not Established
Not Established
Not Established

Engineering Controls:  Avoid creating dust or mist. Local exhaust ventilation, process enclosures, or other engineering controls are required when handling or using this product to avoid over exposure. Use explosion-proof ventilation equipment. Do not use in closed or confined spaces. Keep all levels below exposure limits. Perform regular monitoring to ensure exposure limits are not exceeded.

Personal Protective Equipment (PPE):

Respiratory Protection - Do not breathe vapors. When concentrations exceed the established limits, wear an appropriate, properly fitted respirator (NIOSH/MSHA) until vapors are exhausted. Observe OSHA standard 29 CFR 1910.134 and ANSI Z88.2 requirements whenever workplace conditions require a respirators use.

Hand Protection - Wear appropriate protective gloves and clothing to prevent skin exposure. Gloves must be inspected prior to use. Use proper glove removal technique (without touching gloves outer surface) to avoid skin contact with this product.

Eye Protection - Use safety eyewear with splash guards or side shields. Use additional eye protection such as chemical safety goggles when the possibility for eye contact from splashing, spraying liquid, or airborne material exists.

Skin Protection - Avoid contact with this product. Wear appropriate protective gloves and clothing to prevent skin exposure. Use proper glove and clothing removal techniques to avoid skin contact with this product. When handling large quantities, eye wash stations and deluge showers should be available.

Hygiene Measures:

SDS for:  0365F210
Page 3 of 6
Printed:  6/21/2023 at  4:20:45PM

General - When using do not eat or drink. Wash hands with soap and water before breaks and at the end of each workday.

Contaminated Equipment - Avoid contact with contaminated clothing and protective gear/equipment. Wash before reuse.

SECTION 9:     PHYSICAL AND CHEMICAL PROPERTIES

This mixture typically exhibits the following properties under normal circumstances:
Liquid Dispersion
Appearance
Mild
Odor
Liquid
Physical State
2100 °C
Boiling Point
1.313
Specific Gravity (SG)
0.18
Lbs VOC/Gallon Less Water
SECTION 10:     STABILITY AND REACTIVITY

Product Stability (under normal conditions):
STABLE
Incompatible Materials:  Strong acids, strong bases, oxidizing agents
Hazardous Decomposition Products:  Carbon Dioxide (CO2), Carbon Monoxide (CO), Oxides of Nitrogen (NOx), dense black smoke
Hazardous polymerization will not occur.
SECTION 11:     TOXICOLOGICAL INFORMATION
Mixture Toxicity 
Note - Toxicological studies have not been performed on this mixture. The toxicological data listed is compiled using data from the components of the mixture. Refer to Section 2 of this SDS for GHS classification of acute and chronic effects of exposure.  
Principle Routes of Exposure:
Inhalation		Skin Contact		Eye Contact		Ingestion
May cause damage to the following organs:
Eyes		Skin		Respiratory System		
Carcinogenicity: The following chemicals comprise 0.1% or more of this mixture and are listed and/or classified as carcinogens or potential carcinogens by NTP, IARC, OSHA (mandatory listing) or ACGIH (optional listing):

Carcinogen Rating
CAS Number
Description
% Weight
NIOSH: potential occupational carcinogen
IARC: Possible human carcinogen
OSHA: listed

13463-67-7
Titanium dioxide
10% - 20%
EU REACH: Present (P)

64742-95-6
Solvent naphtha, petroleum, light aromatic
0.1% - 1.0%

SECTION 12:     ECOLOGICAL INFORMATION

Bioaccumulative Potential:  No data available
Mobility in Soil:  No data available
SDS for:  0365F210
Page 4 of 6
Printed:  6/21/2023 at  4:20:45PM

Persistence and Degradability:  No data available

Component Ecotoxicity
Solvent naphtha, petroleum, light aromatic
96 Hr LC50 Oncorhynchus mykiss: 9.22 mg/L
48 Hr EC50 Daphnia magna: 6.14 mg/L
SECTION 13:     DISPOSAL CONSIDERATIONS

Do not discharge product into sewer system. Dispose of in a licensed facility. Waste management should be in full compliance with federal, state, and local laws.

The transportation, storage, treatment and disposal of RCRA waste material must be conducted in compliance with 40 CFR 262, 263, 264, 268 and 270. Chemical additions, processing, or otherwise altering this material may make the waste management information presented in this SDS incomplete, inaccurate or otherwise inappropriate.
SECTION 14:     TRANSPORT INFORMATION

This material is classified for transport as follows:
UN Number
Proper Shipping Name
Agency
Packing Group
Hazard Class
U.S. DOT
Not Regulated
SECTION 15:     REGULATORY INFORMATION

Additional regulatory listings where applicable

State of California Proposition 65 (Safe Drinking Water and Toxic Enforcement Act of 1986)  WARNING! This product contains the following substance(s) which are listed by the State of California as carcinogenic, or a reproductive toxin:
13463-67-7  Titanium dioxide  Carcinogen
Clean Air Act, Section 112, Hazardous Air Pollutants (HAPs) (see 40 CFR 61)  This product contains the following substance(s) which are listed as hazardous air pollutants (HAPs) per the Clean Air Act:
- None
Massachusetts Right To Know  This product contains the following toxic or hazardous substance(s) which appear on the Massachusetts Substance List:
13463-67-7  Titanium dioxide
New Jersey Worker and Community Right to Know Hazardous Substance List  The following substance(s) appear on the New Jersey Right to Know Hazardous Substance List:
13463-67-7  Titanium dioxide
Commonwealth of Pennsylvania Worker and Community Right To Know Act  This product contains the following substance(s) which appear on the Pennsylvania Hazardous Substance List:
13463-67-7  Titanium dioxide
Section 313 of Title III of the Superfund Amendments and Reauthorization Act of 1986 (SARA)  This product contains a chemical or chemicals which are subject to the reporting requirements of the Act, and Title 40, of the Code of Federal Regulations, part 372:

- None
Canadian DSL All substances in this product except those listed below are listed or exempt from reporting:
SDS for:  0365F210
Page 5 of 6
Printed:  6/21/2023 at  4:20:45PM

13463-67-7  Titanium dioxide
66402-68-4  Ceramic materials and wares, chemicals
20344-49-4  Iron hydroxide oxide
64742-95-6  Solvent naphtha, petroleum, light aromatic
All Components Listed
Regulation
Country
Canada
Canadian NDSL
No
Australian
Australian Inventory of Chemical Substances
No
Japan
Existing and New Chemical Substances
No
China
Inventory of Existing Chemical Substances Produced or Imported in China
No
New Zealand
Inventory of Chemicals
No
Philippines
Philippine Inventory of Chemicals and Chemical Substances
No
Reach PBT/vPvB
No
TSCA Substance Control Act (TSCA)  All substances except those listed below appear in the Toxic Substances Control Act, Chemical Substance Inventory:

- None
SECTION 16:     OTHER INFORMATION

Disclaimer:  The Volatile Organic Compound (VOC) content reported herein, if any, is based on a material VOC calculation. Several methods are used for the calculation of VOC content, and the standards and requirements regarding VOC content vary by location or jurisdiction.

This document has been prepared using data from sources considered to be technically reliable and is believed to be correct as of the date hereof. It does not constitute a warranty, expressed or implied, as to the accuracy of the information contained herein. Actual conditions of use and handling are beyond the seller's control. User is responsible to evaluate all available information when using product for any particular use, and to comply with all federal, state, provincial, and local laws and regulations.

Revision Notes:
Reviewer Revision  
Date Prepared:  6/21/2023
SDS for:  0365F210
Page 6 of 6
Printed:  6/21/2023 at  4:20:45PM